IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: 7d6d4adf-d8e6-467a-b4b9-725ab84aa43a, NumberOfSaves: 10]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates]"
File name: "Project Number"
Time stamp: "2024-07-15T20:20:29+05:45"
Preprocessor: "ODA SDAI 24.3"
Originating system: "Autodesk Revit 24.1.11.26 (ENU) - IFC 24.1.11.26"
Application: "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)"

People and organizations
  Person "architechplan" of Organization (no name given)
  Owner history of Person "architechplan" of Organization (no name given) | application "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)" | change NOCHANGE | created 1721054108 (2024-07-15T14:35:08Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KIP (conversion based)
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Ground Floor" | long name "Ground Floor" | object type "Level:1/4" Head" | elevation 0.
        contains 74 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384024" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384025" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384026" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384027" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384028" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384029" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384030" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384031" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384032" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384033" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384034" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384035" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384036" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384037" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384038" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384040" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384042" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384043" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:9" Wall" | object type "Basic Wall:9" Wall" | names: "Basic Wall:9" Wall:391966", "Basic Wall:9" Wall:391967", "Basic Wall:9" Wall:437289" (+7 more) | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:9" Wall" | object type "Basic Wall:9" Wall" | names: "Basic Wall:9" Wall:391968", "Basic Wall:9" Wall:391969" | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:5" Wall" | object type "Basic Wall:5" Wall" | names: "Basic Wall:5" Wall:400100", "Basic Wall:5" Wall:400101", "Basic Wall:5" Wall:400102" (+3 more) | material: layers "Basic Wall:5" Wall" ("Wood Planks" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | object type "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | names: "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082" | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | object type "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | names: "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557" | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door" | object type "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door" | names: "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978" | material: materials ("Aluminum", "Cherry") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Window-Casement-Triple-Side-Transom:5'*4' Window" | object type "Window-Casement-Triple-Side-Transom:5'*4' Window" | names: "Window-Casement-Triple-Side-Transom:5'*4' Window:412582", "Window-Casement-Triple-Side-Transom:5'*4' Window:413118" | material: materials ("Metal - Aluminum", "Glass") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window-Sliding-Double:60" x 48"" | object type "Window-Sliding-Double:60" x 48"" | names: "Window-Sliding-Double:60" x 48":419629" | material: materials ("Wood - Stained", "Glass") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | object type "Muntin Pattern_2x2:Muntin Pattern_2x2" | names: "Muntin Pattern_2x2:Muntin Pattern_2x2:419632", "Muntin Pattern_2x2:Muntin Pattern_2x2:419633" | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Exterior-Flat:with Sill" | object type "Trim-Window-Exterior-Flat:with Sill" | names: "Trim-Window-Exterior-Flat:with Sill:419634" | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Interior-Flat:Picture Frame" | object type "Trim-Window-Interior-Flat:Picture Frame" | names: "Trim-Window-Interior-Flat:Picture Frame:419635" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Fixed:ventilation" | object type "Fixed:ventilation" | names: "Fixed:ventilation:428191" | material: materials ("Glass", "Sash") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:5" Slab" | object type "Floor:5" Slab" | FLOOR | names: "Floor:5" Slab:430699" | material: layers "Floor:5" Slab" ("Default Floor" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Concrete-Rectangular Beam:4"*9" Lintel Beam" | object type "Concrete-Rectangular Beam:4"*9" Lintel Beam" | names: "Concrete-Rectangular Beam:4"*9" Lintel Beam:432908" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Concrete-Rectangular Beam:3"*9" Sill Beam" | object type "Concrete-Rectangular Beam:3"*9" Sill Beam" | names: "Concrete-Rectangular Beam:3"*9" Sill Beam:433383" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Concrete-Rectangular Beam:3"*9" Sill Beam" | object type "Concrete-Rectangular Beam:3"*9" Sill Beam" | names: "Concrete-Rectangular Beam:3"*9" Sill Beam:433973" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          3 x IFCROOF | type IFCTYPEPRODUCT "Fascia:Fascia-Flat 1x12" | object type "Fascia:Fascia-Flat 1x12" | names: "Fascia:Fascia-Flat 1x12:437920", "Fascia:Fascia-Flat 1x12:439862", "Fascia:Fascia-Flat 1x12:439902" | parts: 2 IFCSLAB | material: "Gypsum Wall Board" | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Gutter:Gutter - Bevel 5" x 5":45107" | object type "Gutter:Gutter - Bevel 5" x 5"" | names: "Gutter:Gutter - Bevel 5" x 5":439950" | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff, Pset_PipeSegmentTypeGutter
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:10" Wall" | object type "Basic Wall:10" Wall" | names: "Basic Wall:10" Wall:445604", "Basic Wall:10" Wall:445605", "Basic Wall:10" Wall:445606" (+1 more) | material: layers "Basic Wall:10" Wall" ("Cherry" 0.83333333333333337) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | STRAIGHT_RUN_STAIR | names: "Assembled Stair:Stair:449743" | parts: 2 IFCMEMBER, 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | QUARTER_TURN_STAIR | names: "Assembled Stair:Stair:450812" | parts: 6 IFCMEMBER, 2 IFCRAILING, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          3 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | names: "Assembled Stair:Stair:451879", "Assembled Stair:Stair:466585", "Assembled Stair:Stair:468632" | parts: 20 IFCMEMBER, 5 IFCSTAIRFLIGHT, 3 IFCSLAB, 2 IFCRAILING | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | HALF_TURN_STAIR | names: "Assembled Stair:Stair:454125" | parts: 8 IFCMEMBER, 2 IFCRAILING, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | DOUBLE_RETURN_STAIR | names: "Assembled Stair:Stair:455664" | parts: 10 IFCMEMBER, 3 IFCSTAIRFLIGHT, 2 IFCRAILING, 2 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          3 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Default" | object type "Pipe Types:Default" | names: "Pipe Types:Default:457966", "Pipe Types:Default:457981", "Pipe Types:Default:457997" | property sets: Pset_DistributionFlowElementCommon, Pset_DuctConnection, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_PipeConnection, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Elbow - Generic:Standard" | object type "Elbow - Generic:Standard" | names: "Elbow - Generic:Standard:457995", "Elbow - Generic:Standard:458003" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeFittingTypeCommon, Pset_QuantityTakeOff
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | SPIRAL_STAIR | names: "Assembled Stair:Stair:458710", "Assembled Stair:Stair:461180" | parts: 10 IFCMEMBER, 4 IFCRAILING, 3 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCGRID | names: "Default Grid"
        IFCSPACE "1" | long name "Area" | INTERNAL
        IFCSPACE "2" | long name "Area" | INTERNAL
        IFCSPACE "3" | long name "Area" | INTERNAL
        IFCSPACE "4" | long name "Area" | INTERNAL
      IFCBUILDINGSTOREY "First Floor" | long name "First Floor" | object type "Level:1/4" Head" | elevation 9.4166666666682879
        contains 63 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:390995" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:390996" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:390997" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:390998" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:390999" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391000" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391001" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391002" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391003" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391004" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391005" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391006" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391007" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391008" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391009" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391010" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391011" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391012" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          27 x IFCBEAM | type IFCBEAMTYPE "Concrete-Rectangular Beam:12*14 Beam" | object type "Concrete-Rectangular Beam:12*14 Beam" | names: "Concrete-Rectangular Beam:12*14 Beam:391416", "Concrete-Rectangular Beam:12*14 Beam:391418", "Concrete-Rectangular Beam:12*14 Beam:391419" (+24 more) | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:9" Wall" | object type "Basic Wall:9" Wall" | names: "Basic Wall:9" Wall:392171", "Basic Wall:9" Wall:392388", "Basic Wall:9" Wall:392564" (+1 more) | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:5" Wall" | object type "Basic Wall:5" Wall" | names: "Basic Wall:5" Wall:397961", "Basic Wall:5" Wall:398200", "Basic Wall:5" Wall:398419" (+3 more) | material: layers "Basic Wall:5" Wall" ("Wood Planks" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCSLAB | type IFCSLABTYPE "Floor:5" Slab" | object type "Floor:5" Slab" | FLOOR | names: "Floor:5" Slab:430632", "Floor:5" Slab:476488" | material: layers "Floor:5" Slab" ("Default Floor" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCROOF | object type "Basic Roof:5" Roof" | names: "Basic Roof:5" Roof:437772" | parts: 6 IFCSLAB | material: layers "Basic Roof:5" Roof" ("Default Roof" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Roof Soffit:Generic - 4"" | object type "Roof Soffit:Generic - 4"" | CEILING | names: "Roof Soffit:Generic - 4":437972", "Roof Soffit:Generic - 4":438751", "Roof Soffit:Generic - 4":438988" | material: layers "Roof Soffit:Generic - 4"" ("Door - Frame" 0.33333333333333331) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCRAILING | type IFCRAILINGTYPE "Railing:Handrail - Rectangular" | object type "Railing:Handrail - Rectangular" | names: "Railing:Handrail - Rectangular:476533" | material: "<Unnamed>" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Second Floor" | long name "Second Floor" | object type "Level:Level" | elevation 18.833333333333574
        contains 32 elements
          18 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:391017", "Concrete-Rectangular-Column:12*12 Column:391018", "Concrete-Rectangular-Column:12*12 Column:391019" (+15 more) | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:9" Wall" | object type "Basic Wall:9" Wall" | names: "Basic Wall:9" Wall:395049", "Basic Wall:9" Wall:395050", "Basic Wall:9" Wall:395051" (+1 more) | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:5" Wall" | object type "Basic Wall:5" Wall" | names: "Basic Wall:5" Wall:400108", "Basic Wall:5" Wall:400109", "Basic Wall:5" Wall:400110" (+5 more) | material: layers "Basic Wall:5" Wall" ("Wood Planks" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:5" Slab" | object type "Floor:5" Slab" | FLOOR | names: "Floor:5" Slab:430684" | material: layers "Floor:5" Slab" ("Default Floor" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Third Floor" | long name "Third Floor" | object type "Level:Level" | elevation 28.250000000001862
        contains 10 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:5" Slab" | object type "Floor:5" Slab" | FLOOR | names: "Floor:5" Slab:439995" | material: layers "Floor:5" Slab" ("Default Floor" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Parapet Wall" | object type "Basic Wall:Parapet Wall" | names: "Basic Wall:Parapet Wall:440659", "Basic Wall:Parapet Wall:440660", "Basic Wall:Parapet Wall:440661" (+1 more) | material: layers "Basic Wall:Parapet Wall" ("Default Wall" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "441129" | names: "441129" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "441130" | names: "441130" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "441131" | names: "441131" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "441132" | names: "441132" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCGRID | names: "Default Grid"

Types
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCWALLTYPE "Basic Wall:9" Wall" | STANDARD | 20 occurrences | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:5" Wall" | STANDARD | 20 occurrences | material: layers "Basic Wall:5" Wall" ("Wood Planks" 0.41666666666666669) | property sets: Pset_WallCommon
  IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | 1 occurrence | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082, Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082:1, Pset_DoorCommon
  IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | 1 occurrence | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557, Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557:1, Pset_DoorCommon
  IFCDOORSTYLE "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Aluminum", "Cherry") | property sets: Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978, Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978:1, Pset_DoorCommon
  IFCWINDOWSTYLE "Window-Casement-Triple-Side-Transom:5'*4' Window" | 2 occurrences | material: materials ("Metal - Aluminum", "Glass") | property sets: Window-Casement-Triple-Side-Transom:5'*4' Window:412582, Pset_WindowCommon
  IFCWINDOWSTYLE "Window-Sliding-Double:60" x 48"" | 1 occurrence | material: materials ("Wood - Stained", "Glass") | property sets: Window-Sliding-Double:60" x 48":419629, Pset_WindowCommon
  IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | 2 occurrences | material: materials ("Clad - White", "Wood - Stained")
  IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Exterior-Flat:with Sill" | 1 occurrence | material: "Clad - White"
  IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Interior-Flat:Picture Frame" | 1 occurrence | material: "Wood - Stained"
  IFCWINDOWSTYLE "Fixed:ventilation" | 1 occurrence | material: materials ("Glass", "Sash") | property sets: Fixed:ventilation:428191, Pset_WindowCommon
  IFCSLABTYPE "Floor:5" Slab" | FLOOR | 5 occurrences | material: layers "Floor:5" Slab" ("Default Floor" 0.41666666666666669) | property sets: Pset_SlabCommon
  IFCBEAMTYPE "Concrete-Rectangular Beam:4"*9" Lintel Beam" | BEAM | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Concrete-Rectangular Beam:3"*9" Sill Beam" | BEAM | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Concrete-Rectangular Beam:3"*9" Sill Beam" | BEAM | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon
  IFCTYPEPRODUCT "Fascia:Fascia-Flat 1x12" | 3 occurrences
  IFCPIPESEGMENTTYPE "Gutter:Gutter - Bevel 5" x 5":45107" | element type "Gutter:Gutter - Bevel 5" x 5":45107" | GUTTER | 1 occurrence
  IFCWALLTYPE "Basic Wall:10" Wall" | STANDARD | 4 occurrences | material: layers "Basic Wall:10" Wall" ("Cherry" 0.83333333333333337) | property sets: Pset_WallCommon
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 3 occurrences
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCPIPESEGMENTTYPE "Pipe Types:Default" | 3 occurrences
  IFCPIPEFITTINGTYPE "Elbow - Generic:Standard" | 2 occurrences | material: "<Unnamed>"
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 2 occurrences
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "Concrete-Rectangular Beam:12*14 Beam" | 27 occurrences | property sets: Pset_BeamCommon
  IFCCOVERINGTYPE "Roof Soffit:Generic - 4"" | CEILING | 3 occurrences | property sets: Pset_CoveringCommon
  IFCRAILINGTYPE "Railing:Handrail - Rectangular" | 1 occurrence | property sets: Pset_RailingCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 18 occurrences | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCWALLTYPE "Basic Wall:Parapet Wall" | STANDARD | 4 occurrences | material: layers "Basic Wall:Parapet Wall" ("Default Wall" 0.41666666666666669) | property sets: Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "441129" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "441130" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "441131" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "441132" | 1 occurrence

Property sets
  Pset_AirSideSystemInformation | properties | on 4 objects (4 IFCSPACE)
    Name = "Area" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ground Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "First Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Second Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Third Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (4 IFCSPACE)
    Name = "Area" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ground Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "First Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Second Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Third Floor" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 1" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 2" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 3" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 4" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 31 objects (31 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 23 objects (23 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 37 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_QuantityTakeOff | properties | on 56 objects (56 IFCMEMBER)
    Reference = "Carriage - 2" Width" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 54 objects (54 IFCCOLUMN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 27 objects (27 IFCBEAM)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 20 objects (18 IFCWALLSTANDARDCASE, 2 IFCWALL)
    Reference = "9" Wall" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    Reference = "5" Wall" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 16 objects (16 IFCSTAIRFLIGHT)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 15 objects (15 IFCRAILING)
    Reference = "Handrail - Rectangular" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (9 IFCSTAIR)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 21 more contents on 61 objects not shown
  Pset_ReinforcementBarPitchOfColumn | properties | on 54 objects (54 IFCCOLUMN)
    Reference = "12*12 Column" (IFCLABEL)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 15. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 9.9999999999999964 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 10.000000000000007 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 15.00000000000005 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 2 objects (2 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "3"*9" Sill Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 39. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8.0000000000000071 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 10. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon: 11 more contents on 10 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 27 objects (27 IFCBEAM)
    Reference = "12*14 Beam" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM)
    Reference = "3"*9" Sill Beam" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM)
    Reference = "4"*9" Lintel Beam" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 20 objects (18 IFCWALLSTANDARDCASE, 2 IFCWALL)
    Reference = "9" Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    Reference = "5" Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Reference = "Parapet Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Reference = "10" Wall" (IFCLABEL)
  Pset_WallCommon | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "5" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 11 objects (9 IFCWALLSTANDARDCASE, 2 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "9" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 9 objects (9 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "9" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Parapet Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "10" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 51.181102362204733 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 1.4173228346456692 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.70866141732283461 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 1 more content on 0 objects not shown
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "3'3"*7' Door" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "3'*7' Door" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "5'*4' Window" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "5'*4' Window" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "60" x 48"" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "ventilation" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 type objects
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.6886000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "with Sill" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Picture Frame" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 8 objects (8 IFCSLAB)
    Reference = "Non-Monolithic Landing" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 6 objects (6 IFCSLAB)
    Reference = "5" Roof" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 5 objects (5 IFCSLAB)
    Reference = "5" Slab" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Fascia-Flat 1x12" (IFCLABEL)
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Non-Monolithic Landing" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 20. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "5" Roof" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 5 objects (5 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "5" Slab" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Fascia-Flat 1x12" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "5" Slab" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 3 objects (3 IFCROOF)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Fascia-Flat 1x12" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 2639.1944444444471 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
    Reference = "5" Roof" (IFCIDENTIFIER)
    TotalArea = 2808.5720650196945 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    Reference = "Generic - 4"" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 0.33333333333333331 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_DistributionFlowElementCommon | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2 objects (2 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWSEGMENT)
    Reference = "Gutter - Bevel 5" x 5"" (IFCIDENTIFIER)
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 201.87500000000006 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 4.3023264645532722 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 2.6046529291065621 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 2.2189931312199125 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 201.87500000000006 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 4.6821765911778463 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 4.3023264645532722 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 2.4665261318168286 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 2.6046529291065621 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 0.23103384236923294 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Length = 2.2189931312199125 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_PipeSegmentTypeGutter | properties | on 1 object (1 IFCFLOWSEGMENT)
    Slope = 69.427670074385659 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 17. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 4. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754627 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 8. (IFCCOUNTMEASURE)
    NumberOfTreads = 7. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754627 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 6. (IFCCOUNTMEASURE)
    NumberOfTreads = 5. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 5. (IFCCOUNTMEASURE)
    NumberOfTreads = 4. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon: 6 more contents on 6 objects not shown
  Pset_MemberCommon | properties | on 55 objects (55 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Carriage - 2" Width" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Carriage - 2" Width" (IFCIDENTIFIER)
    Slope = 73.134131486543495 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_DuctConnection | properties | on 3 objects (3 IFCFLOWSEGMENT)
    ConnectionType = ["Generic"] (IFCTEXT)
  Pset_PipeConnection | properties | on 3 objects (3 IFCFLOWSEGMENT)
    ConnectionType = ["Generic"] (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 2 objects (2 IFCFLOWFITTING)
    NominalDiameter = [0.5] (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_RailingCommon | properties | on 15 objects (15 IFCRAILING)
    Height = 3. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Handrail - Rectangular" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082 | predefined | on 1 type object
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082:1 | predefined | on 1 type object
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557 | predefined | on 1 type object
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557:1 | predefined | on 1 type object
  Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978 | predefined | on 1 type object
  Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978:1 | predefined | on 1 type object
  Window-Casement-Triple-Side-Transom:5'*4' Window:412582 | predefined | on 1 type object
  Window-Sliding-Double:60" x 48":419629 | predefined | on 1 type object
  Fixed:ventilation:428191 | predefined | on 1 type object