IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: 7af5dbae-aa73-4621-9c0e-701a05f6490a, NumberOfSaves: 11]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates]"
File name: "Project Number"
Time stamp: "2024-07-16T20:29:51+05:45"
Preprocessor: "ODA SDAI 24.3"
Originating system: "Autodesk Revit 24.1.11.26 (ENU) - IFC 24.1.11.26"
Application: "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)"

People and organizations
  Person "architechplan" of Organization (no name given)
  Owner history of Person "architechplan" of Organization (no name given) | application "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)" | change NOCHANGE | created 1721141072 (2024-07-16T14:44:32Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KIP (conversion based)
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Ground Floor" | long name "Ground Floor" | object type "Level:1/4" Head" | elevation 0.
        contains 61 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384024" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384025" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384026" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384027" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384028" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384029" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384030" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384031" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384032" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384033" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384034" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384035" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384036" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384037" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384038" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384040" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384042" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384043" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:9" Wall" | object type "Basic Wall:9" Wall" | names: "Basic Wall:9" Wall:391966", "Basic Wall:9" Wall:391967" | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:9" Wall" | object type "Basic Wall:9" Wall" | names: "Basic Wall:9" Wall:391968", "Basic Wall:9" Wall:391969" | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:5" Wall" | object type "Basic Wall:5" Wall" | names: "Basic Wall:5" Wall:400100", "Basic Wall:5" Wall:400101", "Basic Wall:5" Wall:400102" (+5 more) | material: layers "Basic Wall:5" Wall" ("Wood Planks" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | object type "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | names: "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082" | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | object type "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | names: "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557" | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door" | object type "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door" | names: "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978" | material: materials ("Aluminum", "Cherry") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Window-Casement-Triple-Side-Transom:5'*4' Window" | object type "Window-Casement-Triple-Side-Transom:5'*4' Window" | names: "Window-Casement-Triple-Side-Transom:5'*4' Window:412582", "Window-Casement-Triple-Side-Transom:5'*4' Window:413118" | material: materials ("Metal - Aluminum", "Glass") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window-Sliding-Double:60" x 48"" | object type "Window-Sliding-Double:60" x 48"" | names: "Window-Sliding-Double:60" x 48":419629" | material: materials ("Wood - Stained", "Glass") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | object type "Muntin Pattern_2x2:Muntin Pattern_2x2" | names: "Muntin Pattern_2x2:Muntin Pattern_2x2:419632", "Muntin Pattern_2x2:Muntin Pattern_2x2:419633" | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Exterior-Flat:with Sill" | object type "Trim-Window-Exterior-Flat:with Sill" | names: "Trim-Window-Exterior-Flat:with Sill:419634" | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Interior-Flat:Picture Frame" | object type "Trim-Window-Interior-Flat:Picture Frame" | names: "Trim-Window-Interior-Flat:Picture Frame:419635" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Fixed:ventilation" | object type "Fixed:ventilation" | names: "Fixed:ventilation:428191" | material: materials ("Glass", "Sash") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Concrete-Rectangular Beam:4"*9" Lintel Beam" | object type "Concrete-Rectangular Beam:4"*9" Lintel Beam" | names: "Concrete-Rectangular Beam:4"*9" Lintel Beam:432908" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Concrete-Rectangular Beam:3"*9" Sill Beam" | object type "Concrete-Rectangular Beam:3"*9" Sill Beam" | names: "Concrete-Rectangular Beam:3"*9" Sill Beam:433383" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | STRAIGHT_RUN_STAIR | names: "Assembled Stair:Stair:449743" | parts: 2 IFCMEMBER, 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | QUARTER_TURN_STAIR | names: "Assembled Stair:Stair:450812" | parts: 6 IFCMEMBER, 2 IFCRAILING, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          3 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | names: "Assembled Stair:Stair:451879", "Assembled Stair:Stair:466585", "Assembled Stair:Stair:468632" | parts: 20 IFCMEMBER, 5 IFCSTAIRFLIGHT, 4 IFCRAILING, 3 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | HALF_TURN_STAIR | names: "Assembled Stair:Stair:454125" | parts: 8 IFCMEMBER, 2 IFCRAILING, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | DOUBLE_RETURN_STAIR | names: "Assembled Stair:Stair:455664" | parts: 10 IFCMEMBER, 3 IFCSTAIRFLIGHT, 2 IFCRAILING, 2 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          2 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | SPIRAL_STAIR | names: "Assembled Stair:Stair:458710", "Assembled Stair:Stair:461180" | parts: 10 IFCMEMBER, 4 IFCRAILING, 3 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Cast-In-Place Stair:Monolithic Stair" | object type "Cast-In-Place Stair:Monolithic Stair" | names: "Cast-In-Place Stair:Stair:480082" | parts: 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          6 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:2' x 4' ACT System" | object type "Compound Ceiling:2' x 4' ACT System" | CEILING | names: "Compound Ceiling:2' x 4' ACT System:480754", "Compound Ceiling:2' x 4' ACT System:480762", "Compound Ceiling:2' x 4' ACT System:480774" (+3 more) | material: layers "Compound Ceiling:2' x 4' ACT System" ("ceiling" 0.13541666666666666, "ceiling" 0.052083333333333336) | property sets: Pset_CoveringCommon, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:5" Wall" | object type "Basic Wall:5" Wall" | names: "Basic Wall:5" Wall:483715" | material: layers "Basic Wall:5" Wall" ("Wood Planks" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Curtain Wall 1" | object type "Curtain Wall:Curtain Wall 1" | names: "Curtain Wall:Curtain Wall 1:484578" | parts: 87 IFCMEMBER, 30 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
        IFCSPACE "1" | long name "Area" | INTERNAL
        IFCSPACE "2" | long name "Area" | INTERNAL
        IFCSPACE "3" | long name "Area" | INTERNAL
        IFCSPACE "4" | long name "Area" | INTERNAL
      IFCBUILDINGSTOREY "First Floor" | long name "First Floor" | object type "Level:1/4" Head" | elevation 9.4166666666682879
        contains 27 elements
          27 x IFCBEAM | type IFCBEAMTYPE "Concrete-Rectangular Beam:12*14 Beam" | object type "Concrete-Rectangular Beam:12*14 Beam" | names: "Concrete-Rectangular Beam:12*14 Beam:391416", "Concrete-Rectangular Beam:12*14 Beam:391418", "Concrete-Rectangular Beam:12*14 Beam:391419" (+24 more) | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
      IFCBUILDINGSTOREY "Second Floor" | long name "Second Floor" | object type "Level:Level" | elevation 18.833333333333574
      IFCBUILDINGSTOREY "Third Floor" | long name "Third Floor" | object type "Level:Level" | elevation 28.250000000001862

Types
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCWALLTYPE "Basic Wall:9" Wall" | STANDARD | 4 occurrences | material: layers "Basic Wall:9" Wall" ("Pink Paint" 0.041666666666666664, "Default Wall" 0.75, "Gypsum Wall Board" 0.041666666666666664) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:5" Wall" | STANDARD | 9 occurrences | material: layers "Basic Wall:5" Wall" ("Wood Planks" 0.41666666666666669) | property sets: Pset_WallCommon
  IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | 1 occurrence | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082, Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082:1, Pset_DoorCommon
  IFCDOORSTYLE "Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door" | 1 occurrence | material: materials ("Cherry", "Aluminum", "Glass") | property sets: Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557, Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557:1, Pset_DoorCommon
  IFCDOORSTYLE "Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Aluminum", "Cherry") | property sets: Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978, Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978:1, Pset_DoorCommon
  IFCWINDOWSTYLE "Window-Casement-Triple-Side-Transom:5'*4' Window" | 2 occurrences | material: materials ("Metal - Aluminum", "Glass") | property sets: Window-Casement-Triple-Side-Transom:5'*4' Window:412582, Pset_WindowCommon
  IFCWINDOWSTYLE "Window-Sliding-Double:60" x 48"" | 1 occurrence | material: materials ("Wood - Stained", "Glass") | property sets: Window-Sliding-Double:60" x 48":419629, Pset_WindowCommon
  IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | 2 occurrences | material: materials ("Clad - White", "Wood - Stained")
  IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Exterior-Flat:with Sill" | 1 occurrence | material: "Clad - White"
  IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Interior-Flat:Picture Frame" | 1 occurrence | material: "Wood - Stained"
  IFCWINDOWSTYLE "Fixed:ventilation" | 1 occurrence | material: materials ("Glass", "Sash") | property sets: Fixed:ventilation:428191, Pset_WindowCommon
  IFCBEAMTYPE "Concrete-Rectangular Beam:4"*9" Lintel Beam" | BEAM | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Concrete-Rectangular Beam:3"*9" Sill Beam" | BEAM | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_BeamCommon
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 3 occurrences
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 2 occurrences
  IFCTYPEPRODUCT "Cast-In-Place Stair:Monolithic Stair" | 1 occurrence
  IFCCOVERINGTYPE "Compound Ceiling:2' x 4' ACT System" | CEILING | 6 occurrences | property sets: Pset_CoveringCommon
  IFCCURTAINWALLTYPE "Curtain Wall:Curtain Wall 1" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCBEAMTYPE "Concrete-Rectangular Beam:12*14 Beam" | 27 occurrences | property sets: Pset_BeamCommon

Property sets
  Pset_AirSideSystemInformation | properties | on 4 objects (4 IFCSPACE)
    Name = "Area" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ground Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "First Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Second Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Third Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (4 IFCSPACE)
    Name = "Area" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ground Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "First Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Second Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Third Floor" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 1" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 2" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 3" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Area 4" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 10 objects (10 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 18 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_QuantityTakeOff | properties | on 87 objects (87 IFCMEMBER)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 56 objects (56 IFCMEMBER)
    Reference = "Carriage - 2" Width" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 30 objects (30 IFCPLATE)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 27 objects (27 IFCBEAM)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 18 objects (18 IFCCOLUMN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 18 objects (18 IFCRAILING)
    Reference = "Handrail - Rectangular" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 16 objects (16 IFCSTAIRFLIGHT)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (8 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Reference = "5" Wall" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 17 more contents on 43 objects not shown
  Pset_ReinforcementBarPitchOfColumn | properties | on 18 objects (18 IFCCOLUMN)
    Reference = "12*12 Column" (IFCLABEL)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 15. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 9.9999999999999964 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 10.000000000000007 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 15.00000000000005 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8.0000000000000071 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 8. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 10. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*14 Beam" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 9.9999999999999929 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon: 11 more contents on 10 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 27 objects (27 IFCBEAM)
    Reference = "12*14 Beam" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM)
    Reference = "4"*9" Lintel Beam" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 1 object (1 IFCBEAM)
    Reference = "3"*9" Sill Beam" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 9 objects (8 IFCWALLSTANDARDCASE, 1 IFCWALL)
    Reference = "5" Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (2 IFCWALL, 2 IFCWALLSTANDARDCASE)
    Reference = "9" Wall" (IFCLABEL)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "5" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (2 IFCWALL, 2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "9" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "5" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 51.181102362204733 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 1.4173228346456692 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "3'3"*7' Door" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "3'*7' Door" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "5'*4' Window" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "5'*4' Window" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "60" x 48"" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "ventilation" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 type objects
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.6886000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "with Sill" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Picture Frame" (IFCIDENTIFIER)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 17. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "Monolithic Stair" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 4. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754627 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 17. (IFCCOUNTMEASURE)
    NumberOfTreads = 16. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.52314814814823818 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 8. (IFCCOUNTMEASURE)
    NumberOfTreads = 7. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754627 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 9. (IFCCOUNTMEASURE)
    NumberOfTreads = 8. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 6. (IFCCOUNTMEASURE)
    NumberOfTreads = 5. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 5. (IFCCOUNTMEASURE)
    NumberOfTreads = 4. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.55392156862754638 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 1. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.75 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon: 7 more contents on 7 objects not shown
  Pset_MemberCommon | properties | on 55 objects (55 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Carriage - 2" Width" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 16 objects (16 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
    Span = 1.3958333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 11 objects (11 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
    Span = 1.2916666666666665 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 10 objects (10 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
    Span = 1.5 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
    Span = 0.70833333333360304 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 5 objects (5 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
    Span = 1.0000000000000002 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
    Span = 2.791666666666667 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 4 objects (4 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2.5" x 5" rectangular" (IFCIDENTIFIER)
    Span = 0.72222222222222143 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon: 12 more contents on 32 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 8 objects (8 IFCSLAB)
    Reference = "Non-Monolithic Landing" (IFCLABEL)
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Non-Monolithic Landing" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 6 objects (6 IFCCOVERING)
    Finish = "ceiling;" (IFCTEXT)
    Reference = "2' x 4' ACT System" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 type object
    TotalThickness = 0.1875 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Curtain Wall 1" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_PlateCommon | properties | on 30 objects (30 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 18 objects (18 IFCRAILING)
    Height = 3. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Handrail - Rectangular" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 4 objects (4 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082 | predefined | on 1 type object
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404082:1 | predefined | on 1 type object
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557 | predefined | on 1 type object
  Door-Exterior-Single-Entry-Half Flat Glass-Wood_Clad:3'3"*7' Door:404557:1 | predefined | on 1 type object
  Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978 | predefined | on 1 type object
  Door-Interior-Single-5_Panel_Vert-Wood:3'*7' Door:407978:1 | predefined | on 1 type object
  Window-Casement-Triple-Side-Transom:5'*4' Window:412582 | predefined | on 1 type object
  Window-Sliding-Double:60" x 48":419629 | predefined | on 1 type object
  Fixed:ventilation:428191 | predefined | on 1 type object