IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: 61607e32-527f-4085-88f6-d26130747923, NumberOfSaves: 1]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates]"
File name: "Project Number"
Time stamp: "2024-07-21T20:51:40+05:45"
Preprocessor: "ODA SDAI 24.3"
Originating system: "Autodesk Revit 24.1.11.26 (ENU) - IFC 24.1.11.26"
Application: "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)"

People and organizations
  Person "architechplan" of Organization (no name given)
  Owner history of Person "architechplan" of Organization (no name given) | application "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)" | change NOCHANGE | created 1721574375 (2024-07-21T15:06:15Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KIP (conversion based)
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:1/4" Head" | elevation 0.
        contains 36 elements
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:9" Wall" | object type "Basic Wall:9" Wall" | names: "Basic Wall:9" Wall:373970", "Basic Wall:9" Wall:375479", "Basic Wall:9" Wall:375483" (+8 more) | material: layers "Basic Wall:9" Wall" ("Exterior Wall" 0.75) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          12 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:9*9 Column" | object type "Concrete-Rectangular-Column:9*9 Column" | names: "Concrete-Rectangular-Column:9*9 Column:375293", "Concrete-Rectangular-Column:9*9 Column:375294", "Concrete-Rectangular-Column:9*9 Column:375295" (+9 more) | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCDOOR | type IFCDOORSTYLE "Single-Flush:3'*7' D1" | object type "Single-Flush:3'*7' D1" | names: "Single-Flush:3'*7' D1:376602" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Window-Double-Hung-Double:4'*5' W" | object type "Window-Double-Hung-Double:4'*5' W" | names: "Window-Double-Hung-Double:4'*5' W:382499" | material: materials ("Wood - Stained", "Glass") | property sets: Pset_QuantityTakeOff, Pset_WindowCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | object type "Muntin Pattern_2x2:Muntin Pattern_2x2" | names: "Muntin Pattern_2x2:Muntin Pattern_2x2:382502", "Muntin Pattern_2x2:Muntin Pattern_2x2:382503" | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | object type "Muntin Pattern_2x2:Muntin Pattern_2x2" | names: "Muntin Pattern_2x2:Muntin Pattern_2x2:382504", "Muntin Pattern_2x2:Muntin Pattern_2x2:382505" | material: materials ("Clad - White", "Wood - Stained") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Exterior-Flat:with Sill" | object type "Trim-Window-Exterior-Flat:with Sill" | names: "Trim-Window-Exterior-Flat:with Sill:382506" | material: "Clad - White" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Interior-Flat:Picture Frame" | object type "Trim-Window-Interior-Flat:Picture Frame" | names: "Trim-Window-Interior-Flat:Picture Frame:382507" | material: "Wood - Stained" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:5" Wall" | object type "Basic Wall:5" Wall" | names: "Basic Wall:5" Wall:383788", "Basic Wall:5" Wall:384257" | material: layers "Basic Wall:5" Wall" ("Clad - White" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:5" Slab" | object type "Floor:5" Slab" | FLOOR | names: "Floor:5" Slab:384789" | material: layers "Floor:5" Slab" ("Clad - White" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | object type "Assembled Stair:7" max riser 11" tread" | HALF_TURN_STAIR | names: "Assembled Stair:Stair:385185" | parts: 3 IFCMEMBER, 2 IFCRAILING, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:1/4" Head" | elevation 9.4166666666683358
        contains 2 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:5" Slab" | object type "Floor:5" Slab" | FLOOR | names: "Floor:5" Slab:384842" | material: layers "Floor:5" Slab" ("Clad - White" 0.41666666666666669) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Level 3" | long name "Level 3" | object type "Level:1/4" Head" | elevation 18.833333333333574

Types
  IFCWALLTYPE "Basic Wall:9" Wall" | STANDARD | 11 occurrences | material: layers "Basic Wall:9" Wall" ("Exterior Wall" 0.75) | property sets: Pset_WallCommon
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:9*9 Column" | COLUMN | 12 occurrences | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCDOORSTYLE "Single-Flush:3'*7' D1" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Single-Flush:3'*7' D1:376602, Single-Flush:3'*7' D1:376602:1, Pset_DoorCommon
  IFCWINDOWSTYLE "Window-Double-Hung-Double:4'*5' W" | 1 occurrence | material: materials ("Wood - Stained", "Glass") | property sets: Window-Double-Hung-Double:4'*5' W:382499, Pset_WindowCommon
  IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | 2 occurrences | material: materials ("Clad - White", "Wood - Stained")
  IFCBUILDINGELEMENTPROXYTYPE "Muntin Pattern_2x2:Muntin Pattern_2x2" | 2 occurrences | material: materials ("Clad - White", "Wood - Stained")
  IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Exterior-Flat:with Sill" | 1 occurrence | material: "Clad - White"
  IFCBUILDINGELEMENTPROXYTYPE "Trim-Window-Interior-Flat:Picture Frame" | 1 occurrence | material: "Wood - Stained"
  IFCWALLTYPE "Basic Wall:5" Wall" | STANDARD | 2 occurrences | material: layers "Basic Wall:5" Wall" ("Clad - White" 0.41666666666666669) | property sets: Pset_WallCommon
  IFCSLABTYPE "Floor:5" Slab" | FLOOR | 2 occurrences | material: layers "Floor:5" Slab" ("Clad - White" 0.41666666666666669) | property sets: Pset_SlabCommon
  IFCTYPEPRODUCT "Assembled Stair:7" max riser 11" tread" | 1 occurrence

Property sets
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCCOLUMN)
    Reference = "9*9 Column" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 11 objects (11 IFCWALLSTANDARDCASE)
    Reference = "9" Wall" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (2 IFCSLAB, 1 IFCOPENINGELEMENT)
    Reference = "5" Slab" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCMEMBER)
    Reference = "Stringer - 2" Width" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCDOOR, 1 IFCOPENINGELEMENT)
    Reference = "3'*7' D1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Reference = "5" Wall" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 6 more contents on 7 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 11 objects (11 IFCWALLSTANDARDCASE)
    Reference = "9" Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Reference = "5" Wall" (IFCLABEL)
  Pset_WallCommon | properties | on 11 objects (11 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "9" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "5" Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_ColumnCommon | properties | on 12 objects (12 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "9*9 Column" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfColumn | properties | on 12 objects (12 IFCCOLUMN)
    Reference = "9*9 Column" (IFCLABEL)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "3'*7' D1" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "5" Slab" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "3'*7' D1" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.7021000000000002 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "4'*5' W" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 type object
    FireRating = "0.5h" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.1292907393000005 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Reference = "Muntin Pattern_2x2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "with Sill" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Picture Frame" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "5" Slab" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Non-Monolithic Landing" (IFCLABEL)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "5" Slab" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Non-Monolithic Landing" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 16. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    Reference = "7" max riser 11" tread" (IFCIDENTIFIER)
    RiserHeight = 0.58854166666677099 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.83333333333333337 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0.083333333333333329 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    NumberOfRiser = 8. (IFCCOUNTMEASURE)
    NumberOfTreads = 7. (IFCCOUNTMEASURE)
    Reference = "2" Tread 1" Nosing 1/4" Riser" (IFCIDENTIFIER)
    RiserHeight = 0.58854166666677099 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLength = 0.83333333333333337 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtInnerSide = 0.83333333333333337 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    TreadLengthAtOffset = 0.83333333333333337 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    WalkingLineOffset = 1.7083333333333333 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 2" Width" (IFCIDENTIFIER)
    Slope = 35.231649832369136 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 2" Width" (IFCIDENTIFIER)
    Slope = 35.231649832369158 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 2" Width" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 2 objects (2 IFCRAILING)
    Height = 3. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Handrail - Rectangular" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 3" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 3" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
  Single-Flush:3'*7' D1:376602 | predefined | on 1 type object
  Single-Flush:3'*7' D1:376602:1 | predefined | on 1 type object
  Window-Double-Hung-Double:4'*5' W:382499 | predefined | on 1 type object