IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: 06ea1d4e-8dc8-49f0-b4b2-36fd07914592, NumberOfSaves: 3]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates]"
File name: "Project Number"
Time stamp: "2024-07-06T23:13:35+05:45"
Preprocessor: "ODA SDAI 24.3"
Originating system: "Autodesk Revit 24.1.11.26 (ENU) - IFC 24.1.11.26"
Application: "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)"

People and organizations
  Person "architechplan" of Organization (no name given)
  Owner history of Person "architechplan" of Organization (no name given) | application "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)" | change NOCHANGE | created 1720286884 (2024-07-06T17:28:04Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KIP (conversion based)
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Ground Floor" | long name "Ground Floor" | object type "Level:1/4" Head" | elevation 0.
        contains 19 elements
          18 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | object type "Concrete-Rectangular-Column:12*12 Column" | names: "Concrete-Rectangular-Column:12*12 Column:384024", "Concrete-Rectangular-Column:12*12 Column:384025", "Concrete-Rectangular-Column:12*12 Column:384026" (+15 more) | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "First Floor" | long name "First Floor" | object type "Level:1/4" Head" | elevation 9.4166666666682879
        contains 1 element
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "Second Floor" | long name "Second Floor" | object type "Level:Level" | elevation 18.833333333333574
        contains 1 element
          1 x IFCGRID | names: "Default Grid"

Types
  IFCCOLUMNTYPE "Concrete-Rectangular-Column:12*12 Column" | COLUMN | 18 occurrences | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon

Property sets
  Pset_ColumnCommon | properties | on 18 objects (18 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_QuantityTakeOff | properties | on 18 objects (18 IFCCOLUMN)
    Reference = "12*12 Column" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 18 objects (18 IFCCOLUMN)
    Reference = "12*12 Column" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ground Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "First Floor" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Second Floor" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Ground Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "First Floor" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Second Floor" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)